#!/bin/sh

[ ifup = "$ACTION" ] && [ "$INTERFACE" = "lan" ] && {
    net_mode=$(uci -q get xiaoqiang.common.NETMODE)
    if [ $net_mode == "lanapmode" ]; then
	#  This would forward any multicast packets to all ports allowing your TV to find your DLNA capable NAS with movies
	echo "0" > /sys/devices/virtual/net/br-lan/bridge/multicast_snooping
    fi
}
